#!/bin/sh

#
# This code belongs to https://github.com/elvis-epx/sdr
# No licence information is provided.
#


#./example.py | ./fm1s.py | sox -t raw -r 50000 -b 16 -c 2 -L -e signed-integer - -d

#./example.py > buffer.iq
#./demo.py > sdrplay_buffer.iq
./fm1s_2.py < sdrplay_buffer.iq


# Run the radio direct to audio. Something about 1M samples and 50000 output rate sounds ass, but it works
#rtl_sdr -f 105.5M -s 1M - | ./fm1s.py | sox -t raw -r 50000 -b 16 -c 2 -L -e signed-integer - -d

# Get data from the nooelec device
#rtl_sdr -f 105.5M -s 1M -n 10000 nooelec_buffer.iq
./fm1s.py < nooelec_buffer.iq